Specifications
				
TENT42 - TENT, MULTIPURPOSE, 42m² - Light Weight Frame Hub Tent			
General description
42m² multipurpose tent which can be used for storage, hospital, dispensary, school, office, or other activities. Should have a frame with bottom/floor pipe for easy setup on hard floor. It should also possess a good ventilation system and be comfortable in all climates.	
The tent:
Should have a minimum shelf life of about 5 years.				
Once erected its life span should be at least 1 year				
Flame retardant  CPAI 84 Section 6 (max. afterflame avg 10s)			Comment by Kalle Wessel: Gibt es hierzu einen Standard/Norm? Wenn ja (s.u.), dann die entsprechende auch benennen 	Comment by Imad El-Hayek: No standard available for the disinfection. These specifications are based on our previous procurements.
It should be disinfected easily  , not sensitive to fungi/mould.
		
should be equipped with a flooring / ground sheet.				
Should have a good ventilation system				
Available add ons such as the below mentioned should be offered and quoted separately or easy selection. E.g.:				
Innerliner				
Winterization Kit				
Flysheet 				
Flooring				
Partitions				
				
Width: 6.00 m			
Length: 7.00 m			
Eaves height: at least 2.05 m				
Ridge height: at least 2.90 m				
Doors: 2 doors (1 each short 7 gable side)			
Windows: at least 3 on the long side , 2 on the short side.
		
Tent skin and flooring:
The outer tent liner should be woven PE 250 gsm - water, rot and UV proof and fire resistance according to CPAI-84 Section 6. The tent liner panels should be a separated roof, gables and wall panels for easy set up and handling.				
The ground sheet should be made of woven PE 250 gsm - water; rot and UV proof. It should be bath-tub style with min. 15 cm upstanding sides.				
The windows should be 3 layered: roll-up PE flap, fixed mosquito mesh and transparent PVC roll-up flap, 				
The colors of the materials should be: - tent liner: white and the groundsheet: light grey				
Frame 				
Galvanized steel pipe or aluminium frame				

Packaging MEASUREMENTS
DIMENSIONS: 225 x 57 x 72 cm
WEIGHT: ± 240 kg
VOLUME: 0,93 m³

			
TENT18 – TENT, QUICK UP 3x6m, with logo

Scaffolding
	The tent frame should be completely made of anodized aluminum rectangular tubes 
with aluminum connectors. 
To protect the tent roof from chafing, plastic caps should be attached to all parts and 
screws that come into contact with the fabric.

	Should be received with the frame completely pre-assembled and only needed to be 
pulled apart during assembly. 
This is particularly easy with built-in plastic bushings, which also prevent abrasion 
marks. 
The tubes should snap into place independently. All snap connections should be designed 
in such a way that you cannot jam fingers. The legs should ideally be extended in 10 cm 
increments, resulting in passage heights of 1.92 m to 2.32 m.

	
Roof 

	
	
	
	
	
	
	
	
	
	

	Tent roof should be made of polyester fabric 550dtex (240 g/m ²) coated on one side with PU; 
flame-retardant, waterproof and rot resistant.  The roof should connect to the frame by 
means of Velcro. 
It can remain attached to the scaffold after the initial assembly in dismantled condition and 
thus be packed away dry.
The roofs should be white with GRC Logo.

General:

	- pre-assembled 
	
	
	
	
	
	
	
	
	

	- poles completely made of anodized aluminum 
	
	
	
	
	
	
	
	

	- with robust carrying bag 
	
	
	
	
	
	
	
	

	- without side walls 
	
	
	
	
	
	
	
	
	

	- with scissor-grid folding technology 
	
	
	
	
	
	
	
	

	- min. 6 height adjustable supports 
	
	
	
	
	
	
	
	

	- easy to assemble / unfold by max. 2 persons
	
	
	
	
	
	
	
	

	- roof on each of the 2 long sides with 1 x GRC logo (details on logo please see below)

	floor space = 18m² = 6m x 3m
	
	
	
	
	
	
	
	

	headroom = adjustable up to min. 2.02m
	
	
	
	
	
	
	
	

	ridge height = adjustable from min. 3.05m
	
	
	
	
	
	
	
	

	canvas material / roof = white - 100% waterproof polyester fabric / nylon - UV resistant
	
	
	
	
	

	Total weight = max 30KG 
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GRC Logo	Comment by Kalle Wessel: Nur auf dem kleinen Zelt oder auf beiden? Bitte prüfen.
Bitte auch in den Vertrag zur kurzen Leistungsbeschreibung mit aufnehmen, welches Zelt mit Logo auszuliefern ist (inkl. Logo nach Anlage „Spezifikationen“).
"German Red Cross" logo English, 800mm
On both 6m sides, in the middle
Thermal transfer printing
[image: Ein Bild, das Entwurf, Diagramm, Origami, Design enthält.

KI-generierte Inhalte können fehlerhaft sein.]

IMPORTANT NOTE:
For packaging requirements see separate attached sheet with detailed instructions
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