Spezifikation:
Wir benötigen eine Mikrowaage XPR2U von Mettler, die sowohl sehr kleine Proben, als auch großflächige dünne Proben (Targetschichten) mit hoher Präzision messen kann. Eine Ablesbarkeit des Probengewichts auf 0,1 µm ist notwendig bei hoher Wiederholbarkeit von ~ 0,15 µg.
Um auch großflächige Folien genau messen zu können, muss die Waage einen Probenteller von mindestens 25 mm Durchmesser haben.
Um auch im feinsten Wägebereich schnelle Ergebnisse erzielen zu können, ist eine berührungsfreie Bedienung der wichtigsten Bedienfunktionen, sowie ein geeigneter Windschutz der Wägezelle notwendig.
Die Mikrowaage muss möglichst kompakt sein, damit auf dem vorhandenen Wägetisch eine gute Zugänglichkeit des Probenraums gewährleistet ist.
Die Waage muss in der Lage sein, mit der Software LabX von Mettler zu arbeiten, damit eine Vernetzung mit den schon vorhandenen Waagen möglich ist
Zusätzlich wird ein kompatibler Drucker zur direkten Dokumentation benötigt, der mit aktuellen Schnittstellen ausgestattet sein sollte.
Waage mit Zubehör müssen vor Ort im Targetlabor der GSI in Betrieb genommen werden. Die Inbetriebnahme muss im Angebot enthalten sein.


Specifications:
We require a Mettler XPR2U microbalance capable of measuring both very small samples and large, thin samples (target layers) with high precision. The sample weight must be readable to 0.1 µm with high repeatability of ~0.15 µg.
To ensure accurate measurement of large-area films, the balance must have a sample pan with a diameter of at least 25 mm.
To achieve fast results even in the most precise weighing range, contactless operation of the key functions and a suitable wind shield for the load cell are necessary.
The microbalance must be as compact as possible to ensure good accessibility to the sample area on the existing weighing bench.
The balance must be capable of working with Mettler’s LabX software to enable networking with the existing balances.
In addition, a compatible printer is required for direct documentation, which should be equipped with current interfaces.
The balance and its accessories must be commissioned on-site at the GSI target laboratory. Commissioning must be included in the offer.
